{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Dk_Df","Info","Reference"],"not_rendered":{"charts":2,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Dk_Df","index":0,"n_rows":179,"n_cols":7,"rows_kept":179,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Wide-band Debye Dk(f) and Df(f) model"]
[]
[null," ",null,"Sweep:","Plotting:"]
[null,null,null,"Min","Fmin[Hz]",null," "]
[null,4,1000000,0.75,10000]
[null,null,null,"Max","Fmax[Hz]"]
[null,null,null,1.75,1000000000,null," "]
[null,null,null,"Nsweep","m"]
[null,0.02,null,200,{"$f":"-2/PI()*Dk_Fo*Df_Fo","v":-5.0929581789406514E-2}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null," "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["N_steps","n","Freq [Hz]","Dk(f)","Df(f)"]
[100,1,{"$f":"F_min*incr_^(B80-1)","v":10000},{"$f":"Dk_Fo+m_*LN(C80/F_o)","v":4.2345393916414169},{"$f":"Df_Fo*Dk_Fo/D80","v":1.8892255473620695E-2}]
["Incr_",2,{"$f":"F_min*incr_^(B81-1)","v":11233.240329780274},{"$f":"Dk_Fo+m_*LN(C81/F_o)","v":4.2286166797312799},{"$f":"Df_Fo*Dk_Fo/D81","v":1.8918716464289179E-2}]
[{"$f":"10^(LOG(F_max/F_min)/(N_steps-1))","v":1.1233240329780274},3,12618.568830660204,4.2226939678211437,1.8945251682844302E-2]
[null,4,14174.741629268054,4.2167712559110067,1.8971861442058827E-2]
[null,5,15922.827933410923,4.2108485440008696,1.8998546056465213E-2]
[null,6,17886.495290574348,4.2049258320907326,1.9025305842368015E-2]
[null,7,20092.33002565047,4.1990031201805964,1.9052141117856386E-2]
[null,8,22570.197196339202,4.1930804082704594,1.9079052202816686E-2]
[null,9,25353.64493970112,4.1871576963603223,1.9106039418945179E-2]
[null,10,28480.35868435802,4.1812349844501862,1.9133103089760847E-2]
[null,11,31992.671377973835,4.1753122725400491,1.9160243540618349E-2]
[null,12,35938.136638046279,4.1693895606299121,1.9187461098721031E-2]
[null,13,40370.172585965542,4.163466848719775,1.9214756093134069E-2]
[null,14,45348.785081285831,4.1575441368096389,1.9242128854797761E-2]
[null,15,50941.380148163786,4.1516214248995018,1.9269579716540884E-2]
[null,16,57223.676593502176,4.1456987129893648,1.9297109013094178E-2]
[null,17,64280.731172843211,4.1397760010792286,1.9324717081103959E-2]
[null,18,72208.090183854642,4.1338532891690916,1.9352404259145847E-2]
[null,19,81113.083078968717,4.1279305772589545,1.9380170887738603E-2]
[null,20,91116.275611548932,4.1220078653488175,1.940801730935808E-2]
[null,21,102353.10218990262,4.1160851534386813,1.9435943868451308E-2]
[null,22,114975.69953977357,4.1101624415285443,1.9463950911450714E-2]
[null,23,129154.96650148836,4.1042397296184072,1.9492038786788419E-2]
[null,24,145082.87784959399,4.0983170177082711,1.9520207844910695E-2]
[null,25,162975.08346206442,4.092394305798134,1.954845843829257E-2]
[null,26,183073.82802953682,4.086471593887997,1.9576790921452484E-2]
[null,27,205651.23083486516,4.0805488819778599,1.9605205650967145E-2]
[null,28,231012.97000831601,4.0746261700677238,1.9633702985486477E-2]
[null,29,259502.42113997359,4.0687034581575867,1.9662283285748736E-2]
[null,30,291505.30628251773,4.0627807462474497,1.9690946914595692E-2]
[null,31,327454.91628777282,4.0568580343373135,1.9719694236988005E-2]
[null,32,367837.9771828634,4.0509353224271765,1.9748525620020722E-2]
[null,33,413201.24001153372,4.0450126105170394,1.9777441432938893E-2]
[null,34,464158.88336127793,4.0390898986069033,1.980644204715332E-2]
[null,35,521400.82879996853,4.0331671866967662,1.9835527836256493E-2]
[null,36,585702.08180566679,4.0272444747866292,1.986469917603861E-2]
[null,37,657933.22465756803,4.0213217628764921,1.9893956444503758E-2]
[null,38,739072.20335257787,4.015399050966356,1.9923300021886244E-2]
[null,39,830217.56813197455,4.0094763390562189,1.9952730290667086E-2]
[null,40,932603.34688322002,4.0035536271460819,1.998224763559061E-2]
[null,41,1047615.752789665,3.9976309152359453,2.001185244368121E-2]
[null,42,1176811.9524349987,3.9917082033258087,2.0041545104260292E-2]
[null,43,1321941.1484660292,3.9857854914156716,2.0071326008963317E-2]
[null,44,1484968.2622544654,3.979862779505535,2.0101195551757024E-2]
[null,45,1668100.537200059,3.973940067595398,2.0131154128956809E-2]
[null,46,1873817.4228603845,3.9680173556852614,2.0161202139244251E-2]
[null,47,2104904.1445120205,3.9620946437751243,2.0191339983684786E-2]
[null,48,2364489.4126454075,3.9561719318649877,2.0221568065745571E-2]
[null,49,2656087.7829466867,3.9502492199548511,2.0251886791313473E-2]
[null,50,2983647.2402833398,3.9443265080447141,2.0282296568713245E-2]
[null,51,3351602.6509388429,3.9384037961345775,2.0312797808725847E-2]
[null,52,3764935.8067924692,3.9324810842244404,2.0343390924606956E-2]
[null,53,4229242.8743894994,3.9265583723143038,2.0374076332105615E-2]
[null,54,4750810.1621027971,3.9206356604041668,2.0404854449483083E-2]
[null,55,5336699.23120631,3.9147129484940302,2.0435725697531819E-2]
[null,56,5994842.503189411,3.9087902365838936,2.0466690499594677E-2]
[null,57,6734150.6577508217,3.9028675246737565,2.0497749281584252E-2]
[null,58,7564633.27554629,3.8969448127636199,2.0528902472002397E-2]
[null,59,8497534.3590864446,3.8910221008534829,2.0560150501959952E-2]
[null,60,9545484.566618342,3.8850993889433463,2.0591493805196599E-2]
[null,61,10722672.220103234,3.8791766770332097,2.0622932818100959E-2]
[null,62,12045035.402587825,3.8732539651230726,2.0654467979730837E-2]
[null,63,13530477.74579807,3.867331253212936,2.0686099731833649E-2]
[null,64,15199110.829529341,3.861408541302799,2.0717828518867065E-2]
[null,65,17073526.474706911,3.8554858293926624,2.0749654788019815E-2]
[null,66,{"$f":"F_min*incr_^(B145-1)","v":19179102.61672489},{"$f":"Dk_Fo+m_*LN(C145/F_o)","v":3.8495631174825253},{"$f":"Df_Fo*Dk_Fo/D145","v":2.0781578989232705E-2}]
[null,67,21544346.900318842,3.8436404055723887,2.0813601575219817E-2]
[null,68,24201282.647943825,3.8377176936622521,2.0845723001489905E-2]
[null,69,27185882.427329417,3.8317949817521151,2.087794372636801E-2]
[null,70,30538555.088334166,3.8258722698419785,2.0910264211017236E-2]
[null,71,34304692.863149188,3.8199495579318414,2.0942684919460768E-2]
[null,72,38535285.937105305,3.8140268460217048,2.0975206318604066E-2]
[null,73,43287612.810830593,3.8081041341115678,2.1007828878257299E-2]
[null,74,48626015.800653547,3.8021814222014312,2.1040553071157944E-2]
[null,75,54622772.176843435,3.7962587102912946,2.1073379372993639E-2]
[null,76,61359072.734131753,3.7903359983811575,2.1106308262425228E-2]
[null,77,68926121.043496996,3.7844132864710209,2.1139340221110019E-2]
[null,78,77426368.268112734,3.7784905745608839,2.1172475733725278E-2]
[null,79,86974900.261778355,3.7725678626507473,2.1205715287991932E-2]
[null,80,97700995.729922563,3.7666451507406102,2.1239059374698499E-2]
[null,81,109749876.54930565,3.7607224388304736,2.1272508487725238E-2]
[null,82,123284673.94420666,3.754799726920337,2.1306063124068537E-2]
[null,83,138488637.13938737,3.7488770150102,2.1339723783865536E-2]
[null,84,155567614.39304724,3.7429543031000634,2.1373490970418962E-2]
[null,85,174752840.00076845,3.7370315911899263,2.1407365190222225E-2]
[null,86,196304065.00402713,3.7311088792797897,2.1441346952984733E-2]
[null,87,220513073.99030462,3.7251861673696531,2.1475436771657468E-2]
[null,88,247707635.59917119,3.7192634554595161,2.1509635162458792E-2]
[null,89,278255940.22071254,3.7133407435493795,2.1543942644900498E-2]
[null,90,312571584.96882373,3.7074180316392424,2.1578359741814126E-2]
[null,91,351119173.42151326,3.7014953197291058,2.1612886979377514E-2]
[null,92,394420605.9437657,3.6955726078189688,2.1647524887141625E-2]
[null,93,443062145.75838816,3.6896498959088322,2.16822739980576E-2]
[null,94,497702356.43321133,3.6837271839986956,2.1717134848504113E-2]
[null,95,559081018.25122249,3.6778044720885585,2.1752107978314967E-2]
[null,96,628029144.18342543,3.6718817601784219,2.1787193930806935E-2]
[null,97,705480231.07186472,3.6659590482682849,2.182239325280793E-2]
[null,98,792482898.3539176,3.6600363363581483,2.1857706494685384E-2]
[null,99,890215085.44503891,3.6541136244480112,2.1893134210374962E-2]
[null,100,1000000000.0000005,3.6481909125378746,2.1928676957409493E-2]

{"sheet":"Info","index":1,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[null," "]
[]
[]
[]
[]
[null,"Application information and hints:"]
[null,"1., Enter your data in the top highlighted area of worksheet.  Select any of the red parameters and enter your data in the units shown. "]
[null,"2., Blue numbers are calculated output data. Do not overwrite them unless you understand its consequences in the spreadsheet."]
[null,"3., If you click on any of the green buttons, it will initiate the sweep of the particular parameter between the Min and Max relative limits. To run sweeps, the spreadsheet has to allow macros.The speed of sweep can be controlled by the number of sweep steps (Nsweep) parameter."]
[null,"4., The workbook has been tested in Excel 2000, Excel 2003 and Excel 2007.  Note that Excel 2007 runs the macro orders of magnitude slower than earlier versions, even if you (re)save the file in Excel 2007 Macro-enabled workbook."]
[null,"5., There is no error checking of your entered input data. Physically invalid input (e.g., negative frequency) may result in errors and/or meaningless output.  "]
[null,"6.,   For explanatory information, see the worksheet \"Reference\". For suggested input data to look at, use the Workgroup Scenario items. "]
[null,"7.,  If Automatic Recalculation is selected in the Tools/Options menu, numerical and graphical outputs are automatically updated after each new entry."]
[null,"8.,  This file uses dot (.) as separator between the integer and fractional parts of numbers.   Preferences in your Microsoft Excel installation must be set accordingly. "]
[null,"9.,  The calculation part of the worksheets can be viewed and changed if necessary below the input/output areas.  To navigate among cells, you can switch back on the Row and Column Headers and Scroll bars in the Tools/Options menu."]

{"sheet":"Reference","index":2,"n_rows":43,"n_cols":2,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Reference:"]
[null,"Frequency-Domain Characterization of Power Distribution Networks. Artech House, 2007, pp. 106-109.."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Input parameters:"]
[null,"Dk(fo): relative dielectric constant at the fo working frequency [-]"]
[null,"Df(fo): dielectric loss tangent at the fo working frequency [-]"]
[null,"fo: working frequency, where the Dk and Df values are specified [Hz]"]
[null,"Min: unit-less multiplier of the nominal value; used to set the lower sweep range"]
[null,"Max: unit-less multiplier of the nominal value; used to set the upper sweep range"]
[null,"Nsweep: number of steps during sweep.  Can be used to adjust animation speed."]
[null,"Fmin: minimum frequency for the output plots [Hz]"]
[null,"Fmax: highest frequency for the output plots [Hz]"]